**ZCR(Zero Crossing Rate):**

As the name suggests zero-crossing rate is the measure of the rate at which the signal is going through the zeroth line more formally signal is changing positive to negative or vice versa.

Mathematically it can be measured as

zcr =

Where

* **s = signal**
* **T = length of signal**

It can be used for pitch detection algorithms and also for voice activity detection.